
*******************************
README
PIC32MX USB Starter Board
v1.1 kit release
usb_hid_mouse_device_demo
*******************************

The USB HID Mouse Device Demo for PIC32MX Starter Kit.

How to use:
SW1  - Move mouse cursor up   (momentary contact)
SW2  - Move mouse cursor Left (momentary contact)
SW3  - Invert direction of mouse move for SW1 & SW2 (momentary contact)

LED1 - Mouse Connection status (emulation is always enabled)
        LED On       - Mouse emulation enabled
        LED Off      - Only when board is not powered/running
        LED Blinking - Attached to USB
LED2 - Remote Wakeup Status
        LED On  - Remote wakup enabled
        LED Off - Remote wakup disabled
LED3 - Device sleep status
        LED On  - Device is asleep
        LED Off - Device is awake

Additional information:
PIC32MX Starter Kit release notes - ReleaseNotes.html
PIC32MX Starter Board User's Guide - DS61150
