Getting Started: Running the “PIC32MX USB Starter Kit - Mass Storage Host” demo

Required Hardware

Firmware

Running the Demo

## Required Hardware:

To run this project, you will need one of the following sets of hardware:

PIC32MX USB Starter Board (DM320003)

Firmware:

To run this project, you will need to load the corresponding firmware into the device. There are two methods available for loading the demos: Precompiled demos and source code projects.

Precompiled Demos are available in the “<Install Directory>\USB Precompiled Demos” folders. Each demo should be prefaced with the hardware platform it is compiled for. Select the file that matches the hardware that you have and the demo that you want to run. For more information about how to load a precompiled project, please see the “Getting Started – Loading a precompiled demo” guide.

The source code for this demo is available in the <Install Directory>\sample_code\usb_sk_msd_host_demo directory. In this directory you will find all of the user level source and header files as well as project and workspace files. Find the project (*.mcp) or workspace (*.mcw) file. Compile and program the demo code into the hardware platform. For more help on how to compile and program projects, please refer to the MPLAB® IDE help available through the help menu of MPLAB (Help->Topics…->MPLAB IDE).

Running the Demo:

How to use:

1. Connect a USB Thumb Driver to the Type-A receptacle.

2. Press SW1 to enter a command.

3. Enter "Help" (or '?') for a list of commands.

Refer to AN1142 and application-provided help for additional details.

## Trademarks:

The Microchip name and logo, the Microchip logo, MPLAB, and PIC are registered trademarks of Microchip Technology Incorporated in the U.S.A. and other countries.

PICDEM and PICTail are trademarks of Microchip Technology Incorporated in the U.S.A. and other countries.

Microsoft, Windows, and Windows Vista are either registered trademarks or trademarks of Microsoft Corporation in the United States and/or other countries.

SD is a trademark of the SD Association in the U.S.A and other countries