*******************************
usb_generic_host_demo
PIC32MX Starter Kit
release 1.1
12.01.08
*******************************

The USB Generic Host demo for PIC32MX Starter Kit.

How to use:
(Output will appear the MPLAB "Output" window.)
1. Connect a Microchip Generic (AKA Custom) demo to the Type-A USB 
   receptacle on the USB Starter Board.  LED1 will blink.
2. Press SW1 to display temperature and Potentiometer (POT) readings.
3. Press SW2 to light LED3 on the PICDEM(TM) FS USB Demo board (D9 on the 
   Explorer 16 board).
4. Press SW3 to light LED4 on the PICDEM(TM) FS USB Demo Board (D10 on the
   Explorer 16 board).


Additional information:
PIC32MX Starter Kit release notes - ReleaseNotes.html
PIC32MX Starter Board User's Guide - DS61150